## Answer 1.7

#### The voltage levels on the channel are changing at a maximum rate of 4800 times per second depending on the incoming bit patterns. Taking the worst case of the waveform alternately swinging between maximum and minimum values the waveform shape will be that of a squarewave with repetition frequency 2400 Hz. The fundamental frequency is thus also 2400 Hz which equates to the minimum filter bandwidth.